Appendix 6						Publication ref.: 5/2019


TECHNICAL SPECIFICATIONS AND TECHNICAL TENDER

Contracting Authority: FEROPLAST Ltd., Grožnjanska ulica 5, 52460 Buje, Republic of Croatia
Subject of procurement: Procurement of machinery
Publication reference: 5/2019

TECHNICAL TENDER
Tenderers must fill in the column 2 and enter detailed description of the offered goods (words like “compliant” or “yes” are not sufficient). Tenderer must not change the specifications indicated in the column number 1.
For all producers, types of products, standards or norms indicated in technical specifications shall apply „or equivalent“. Eventual accompanying documentation which the Tenderer submits as the supplement to the tender must clearly indicate the models, or options which are offered. Tenders which do not identify precisely models and specifications may be rejected.
Note: Tenderer fills technical specifications only for the group or groups for which the offer is submitted!
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This project is funded by the European Regional Development Fund 
TEHNICAL SPECIFICATIONS
	I
Requiered specifications
	II
Offered specifications

	GROUP 1
	

	1. Straightening and cutting line machine
   Piece: 1

	Parametar / item
	Characteristics 
	

	Entry material - wire
	Ribbed or smooth wire Ø 2 - 7 mm;
Spool
	

	[bookmark: _Hlk533351781]Maximum spools weight
	maximum to 1.200 kg
	

	Wire direction
	wire path from left to right
	

	Raw material
	Spools Ø2,00 - 7,00 mm;
UTS (Ultimate tensile strength) until 750 Mpa
	

	Wire feed speed
	20 - 120 m/min
	

	Minimum cutting length
	minimum 100 mm
	

	Maximum cutting length
	[bookmark: _GoBack]maximum to 5.000 mm
	

	Flatness tolerance
	from 1mm on 2.000 mm
	

	Maximum length tolerance
	± 0.2 mm
	

	Unwinding the wire
	automatic
	

	Additional requests
	· Installation documentation
· instructions for safe operation
· maintenance documentation
· (all in digital format)
	

	Additional documentation
	· Electro scheme
· Pneumatic scheme
· Mechanical parts scheme
· Spare parts list
	

	GROUP 2
	

	1. Wire butt welding machine
Piece: 1

	Parametar / item
	Characteristics 
	

	Power supply
	400 V / 50 Hz
	

	Minimum rated power at 50% ED
	minimum 25 kVA
	

	Minimum clamping force
	minimum 900 daN
	

	Minimum squeeze force
	minimum 350 daN
	

	Additional requests
	· Installation documentation
· instructions for safe operation
· maintenance documentation
· (all in digital format)
	

	Additional documentation
	· Electro scheme
· Pneumatic scheme
· Mechanical parts scheme
· Spare parts list
	

	GROUP 3
	

	1. Machine for electro resistance welding
Piece: 1

	Parametar / item
	Characteristics 
	

	Projection plates throat depth
	minimum 650 mm
	

	Minimum nominal power
	minimum 150 kVA
	

	Electrode stroke
	minimum 100 mm
	

	Additional requests
	· Installation documentation
· instructions for safe operation
· maintenance documentation
· (all in digital format)
	

	Additional documentation
	· Electro scheme
· Pneumatic scheme
· Mechanical parts scheme
· Spare parts list
	

	GROUP 4
	

	1. Salt spray test chamber
Piece: 1

	Parametar / item
	Characteristics 
	

	Salt chamber type
	Possibility to check according ISO 9227 and ISO 6270-2CH or equivalent
	

	Capacity
	minimum 400 liters
	

	Inner dimension
	minimum 1.000 x 600 x 1.000 mm
	

	Wetting and drying
	from 12°C to 50°C
	

	Salt reservoir
	minimum 80 liters
	

	Stand for samples - spiked suspension
	minimum 6 pieces
	

	Certified salt for probes
	minimum 100 kg
	

	Prague loading
	800 mm
	

	Additional requests
	· Noise level – less than 50 dB
· Calibration certifyicate or equivalent
	

	Additional documentation
	· Installation documentation
· instructions for safe operation
· maintenance documentation
· (all in digital format)
	

	GROUP 5
	

	1. Forklift
Piece: 1

	Parametar / item
	Characteristics 
	

	Main power
	LPG (Liquified petroleum gas)
	

	Manipulation
	From the seat
	

	Tires
	filled
	

	Height of the lowered crane
	maximum to 2.300 mm
	

	Free moving fork
	minimum 150 mm
	

	Lift height
		3.200 mm or more
	

	Maximum lifting at the highest lift height
	minimum 1.700 kg
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