LEGRADMETAL GREDIČAK d.o.o. 
OIB / VAT: 07966753508
Adresa / Address: Mokrice 249, Mokrice (Oroslavje)
Broj telefona/e-mail / Phone Number/e-mail: +385 49 284 876; +385 98 1717 817; legradmetal@gmail.com     





1. IZMJENA POZIVA NA DOSTAVU PONUDA / 1st CHANGE OF CALL FOR PROPOSALS


NAZIV NABAVE: Opremanje postojećeg proizvodnog pogona / PROCUREMENT NAME: Equipping of  the existing production plant






 








Mokrice,20.05.2021. 
U Pozivu na dostavu ponuda u poglavlju 6. Rok i adresa za dostavu ponude, dio teksta se mijenja i glasi: / In the Call for proposals in the chapter 6. Deadline and address for tender delivery time, part of the text is changed to read:
Ponuda se dostavlja u zatvorenoj omotnici, osobno ili poštom, najkasnije do 01.06.2021. do 10:00 h na adresu: LEGRADMETAL GREDIČAK d.o.o., Mokrice 249, Mokrice (Grad Oroslavje). / The tender shall be submited in a sealed envelope, in person or by mailno later than 1 June 2021 at 10 AM on address LEGRADMETAL GREDIČAK Ltd, Mokrice 249, Mokrice (Oroslavje).
U Prilogu B – Troškovnik /tehničke specifikacije, grupa 4, dio teksta se se mijenja i glasi: / In Annex B – The bill of of quantities and technical specifications, group 4,  part of the text is changed to read:
	1.
	Stroj za označavanje alata / Tool marking machine

	
	Mogućnost označavanja alata i proizvoda sa šifrom, barkodom i logotipom / Possibility of marking tools and products with code, barcode and logo

	
	Mogućnost označavanja na reflektivnim materijalima / Possibility of marking on reflective materials

	
	Izlazna snaga: 20 - 30 W / Average Power: 20 - 30 W

	
	Radno polje označavanja: 100 x 100 - 180 x 180 / Marking field: 100 x 100 - 180 x 180

	
	Valna dužina laserske zrake: 1050 - 1090 mm / Wavelength: 1050 - 1090 mm

	
	Maksimalna brzina ispisa: 7000 - 12000 mm/s / Maximum print speed: 7000 - 12000 mm/s

	
	Zaštitne naočale za laser / Laser Safety Glasses

	
	Instalacija i kalibracija lasera / Laser installation and calibration

	
	Osnovna obuka za korištenje stroja (na lokaciji kupca): 1 - 2 dana / Basic machine training (at customer's location): 1 - 2 days

	
	Upute za rad i održavanje / Operating and maintenance instructions


Iz Priloga B – Troškovnik/tehničke specifikacije, grupa 4, se izuzima sljedeća stavka: / From Annex B - The bill of of quantities and technical specifications, group 4, the following item is excluded:
	1.
	Stroj za označavanje alata / Tool marking machine

	
	Stacionarna konzola visine: 400 - 500 mm / Stationary console height: 400 - 500 mm





U Prilogu B – Troškovnik /tehničke specifikacije, grupa 5, dio teksta se se mijenja i glasi: / In Annex B – The bill of of quantities and technical specifications, group 5,  part of the text is changed to read:
	1.
	CNC obradni centar / CNC machining center

	
	Simultani 5-osni obradni centar / Simultaneous 5 axis machining center

	
	Kretanje radne osi X: 730 - 900 mm / Travel X axis: 730 - 900 mm

	
	Kretanje radne osi Y: 450 - 500 mm / Travel Y axis: 450 - 500 mm

	
	Kretanje radne osi Z: 470 - 500 mm / Travel Z axis: 470 - 500 mm

	
	Brzi hodovi (posmaci) na X/Y/Z osi: 36 - 50 m/min / Rapid traverse on X/Y/Z axis: 36 - 50 m/min

	
	Maksimalni broj okretaja glavnog vretena: 12000 - 18000 min¯¹ / Spindle speed maximum  12000 - 18000 min¯¹

	
	Maksimalna izlazna snaga glavnog vretena (kontinuirano): 11 - 22 KW / Main spindle motor output (continuous rating): 11 - 22 KW

	
	Kapacitet spremnika alata: 30 - 48 alata / Tool storage capacity: 30 - 48 tools

	
	Sinkronizirano narezivanje navoja / Synchronised tapping

	
	Kompenzacija radijusa alata prilikom 5-osne obrade / Tool radius compensation during 5-axis machining

	
	Visoki pritisak rashladne tekučine kroz vreteno: 5 - 25 bar-a / Hi pressure coolant thru spindle: 5 - 25 bar

	
	Uređaj za odvođenje strugotine / Chip conveyor

	
	Automatsko umjeravanje dužine alata i otkrivanje loma / Automatic tool length measurement and breakage detection

	
	Elektroničko 3D mjerno ticalo / Electronik 3D touch probe

	
	Maksimalna veličina programa: 32 - 128 MB / Maximum program size: 32 - 128 MB

	
	Softverski paket za 5-osno simultano programiranje / Software package for 5-axis simultaneous programming

	
	Softver za kontrolu točnosti stroja / Software for accuracy check of the machine

	
	Mogućnost programiranja i uređivanja programa u EIA/ISO formatu / The ability to programming and edit the program in EIA / ISO format

	
	Mogućnost programiranja 3D obrade na zakrivljenoj površini na temelju nekoliko fiksnih uzoraka (točaka) / The ability to programming the 3D curved surface machining based on several fixed patterns

	
	Pojednostavljeni digitalni 3D model stroja u STP formatu / Simplified digital 3D model of machine in STP format

	
	Prijevoz na adresu kupca / Transport to customers address

	
	Instalacija stroja kod kupca / Machine installation at the customer's location

	
	Osnovna obuka za korištenje stroja (na lokaciji kupca): 5 - 10 dana / Basic machine training (at customer's location): 5 - 10 days

	
	Upute za rad i održavanje / Operating and maintenance instructions




Sve ostale stavke u Pozivu na dostavu ponuda i Troškovniku ostaju nepromijenjene./ All other items in the Call for proposals and the bill of quantities and technical specifications remain unchanged. 	
Prilaže se novi Poziv na dostavu ponuda i Prilog B - Troškovnik / tehničke specifikacije. / A new Call for proposals and Annex B - The bill of quantities and technical specifications are attached.


