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TECHNICAL SPECIFICATIONS


TECHNICAL SPECIFICATION – Circular saw 
Tenderers are required to fill in column 3 with a detailed description of the supplies offered (words such as "compliant" or "yes" are not sufficient). The Tenderer shall not change the specifications stated in column 2.

For all manufacturers, types of products, standards or norms that are set out in the technical specifications applies "or equivalent”. Any supporting documentation which the Tenderer submits to complement the offer shall clearly indicate the models or options being offered. Offers which do not identify precisely the models and specifications may be rejected.
Technical specifications listed in the table in the check-list format represent minimum standard for every single item of the requested specifications and are sole basis for evaluating the technical compliance of the offers. The Tenderer can also offer products that meet higher standards or technical specifications better than the minimum.

In order for the offer to be considered valid, the offered supplies should satisfy all what is requested in the below table Technical specifications. 





	Nr. 
	Requested specifications
	Offered specifications

	I.
	II.
	III.

	1. Circular saw
	Circular saw
Quantity: 1 piece
	

	
	
	Quantity: 

	
	
	Manufacturer:

	
	
	Model:

	
	Parameter / item
	Characteristic
(minimum requirements)
	

	1.1. Technical requirements  
	Cutting length
	3300 mm
	

	
	Maximum saw blade diameter
	Min. 680 mm
	

	
	Saw blade projection
	Min. 215 mm
	

	
	Maximum clamp opening
	Min. 220 mm
	

	
	Maximum book height 
	Min. 200 mm
	

	
	Minimum book height 
	Max. 6 mm
	

	
	Construction height
	Max. 2500 mm
	

	
	Vibration
	Vibration free
	

	
	Moving possibility 
	Servo drive
	

	1.2. Power and speed
	Main saw motor power
	Min. 55 kw
	

	
	Saw travel speed forward
	from 0,1 to 80 m/min
	

	
	Saw travel speed reverse
	Min. 80 m/min
	

	
	Feeder travel speed reverse - rip-cut-saw
	30 m/min
	

	1.3. Accuracy
	Positioning accuracy
	±0,1 mm 
	

	
	Straightness of cut
	±0,1 mm at 3 m cutting length
	

	1.4. Saw parts 
	Main saw blade 
	Automatic cutting length and height adjustment
	

	
	Saw blade monitoring device 
	with sensor
	

	
	Lubrication system for main saw blade
	3 nozzles for lubrication
	

	
	Cleaning system
	Clean-up cut
Automatic central cleaning of guideways from the base machine 
Automatic central cleaning of guideways and rollers from the feeder carriage 
	

	
	Management of chips
	Automatic chip pusher
Extraction system slider 
Chip basket for capturing of chips
	

	
	Circular saw table and addendums to the table
	Fixed operating table and two movable tables with option of ball air valves for easier movement of the material
	

	
	Roller table
	for cutting lengths 330mm
	

	
	Additional devices
	Dust protection device, Cross aligning device, Cross aligning fence
	

	
	Length of the dual guide for feeder
	5000 mm
	

	
	Feeder carriage and break
	Servo drive
Linear brake
	

	
	Pieces of clamps
	Min. 10
	

	
	Protection 
	Central fan, Protection fence, Safety curtain, Grid with door
	

	
	Maintenance of cleanliness 
	Dust extraction system of minimum motor power 15 kw 
	

	1.5. Circular saw software
	Raw material cut management system  
	Includes parameters for different types of boards based on the material types 
	

	
	Remote diagnostic system 
	via Internet
	

	
	System for marking remainders 
	Option of marking the remainders and their further use 
	

	
	Additional systems which can be offered by a Tenderer – selection criteria
	System for label printing and editing with printer 
System for recording of events
	

	1.6. Service 
	Reaction speed - selection criteria
	Max. 48 hours from the failure notification 
	

	1.7. Warranty period
	Minimum warranty period
	12 months
	

	2. Education
	Education of employees for work on circular saw
	10 working days
	



Place and date: 
_________________________								
On behalf of Tenderer: 
________________________________
Name and surname of authorized person
________________________________
 															Signature of authorized person
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