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[bookmark: _Hlk497833352]ANNEX 4 – TECHNICAL SPECIFICATION 

Bag Making Machines/production lines paper carrier bags with flat handles folded outside (2 items/machines)
	No.
	Technical specification - items
	Dimension

	1.
	*Bag width – the machine must be able to do the minimum of
	230 mm

	2.
	*Bag bottom width – the machine must be able to do the minimum of
	80 mm

	3.
	*Tube length – the machine must be able to do the minimum of
	370 mm

	No.
	Technical specification - items
	Range

	4.
	Reel/roll diameter
	From 110 to 130 cm

	5.
	Material core diameter
	From 72 to 78 mm

	6.
	Handle tape width
	From 15 to 20 mm

	7.
	Handle paper width
	From 80 to 110 mm

	8.
	Handle tape - times folded
	From 6 to 8 times

	9.
	Paper patch diameter
	[bookmark: _GoBack]From 110 to 130 cm

	10.
	Cover strip diameter
	From 110 to 130 cm



* A typical machine for each of these items (with * remark) can offer a specific range. Each range has its own lower (minimum) and upper (maximum) part, i.e. dimensions (for example from 100 mm to 200 mm, where 100 mm is the lowest possibility of the machine, and 200 mm is the highest possibility (maximum) of the machine). Within this Annex 4, the lower possibilities of machines, i.e. the lower part of range (minimum), are prescribed. Tenderers are free to offer machines that have the specified dimensions or less for these items, while the upper part (maximum) of the range will be evaluated within the award criteria as prescribed in Call for tender.
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