
                                                                                                                           
Procurement number: 1/2022






ANNEX 2. _1st AMENDMENT


Contracting Authority: CESTE POŽEGA d.o.o. za niskogradnju, Šijačka cesta 1, 34000 Požega, VAT No.: HR 22203757528
The subject of procurement is equipment for the establishment of a mobile plant for the production of ready-mixed concrete.

The subject of the procurement is not divided into groups. The tenderer is obliged to submit a tender that includes the total subject of procurement as defined in the technical specifications. 

All equipment for the establishment of a mobile concrete plant must be new.
Procurement number: 1/2022
TENDER SUBMISSION FORM 
1. TENDERER:

	Consortium (YES / NO)
	
	For the answer "YES", the Tenderer is obliged to fill in the Table 1_Members of consortium

	The Tenderer intends to subcontract one or more subcontractors (YES / NO)
	
	For the answer "YES", the Tenderer is obliged to fill in the Table 2_ information on subcontractors

	Name of the Tenderer
	

	Registered address
	

	VAT No.
	

	IBAN
	

	Person legally authorised for representation 
	

	The Tenderer is in the VAT system
	

	Regular mail delivery address
	

	Contact person of the Tenderer
	

	Telephone
	

	e-mail
	


2. OFFER INFORMATION:
	Offer number
	

	Offer validity date
	

	Price (without VAT) 
	

	VAT amount 
	

	Total price (with VAT) 
	

	Offered deadline for the delivery and montage  (in days)
	


Table 1_ Members of consortium
	Name of the member of a consortium
	Registered address
	VAT No.
	Name and surname of the authorised person
	Part of the contract that relates to a member of the consortia (specify cost items, quantity, percentage and value)

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


As members of the Consortium for the signature and certification of the joint offer and the validation of the procurement contract, we authorize:
	Name of the holder of the joint offer: 
	

	Name of authorized person to sign a joint offer and contract:
	


Member of the Consortium 1:

Name of authorized person: 
_______________________________________________

Signature of authorised person:
__________________________________________     
Stamp

Member of the Consortium 2:

Name of authorized person: 
_______________________________________________

Signature of authorised person: :
__________________________________________          Stamp

	Date: 
	

	Signature of the authorized person to represent the Consortium:
	


 (Must be repeated depending on the number of members of the community)

Table 2_ Information on subcontractors

	Name of the subcontractor
	Registered address
	VAT No.
	IBAN
	The type of goods that the subcontractor will perform

(specify cost items)
	Value of goods without VAT
	Percentage of expense item

(%)

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	Total value of sub-contracted goods, excluding VAT:
	
	

	VAT:
	
	

	Total value of subcontracted goods with VAT:
	
	


3. TECHINCAL SPECIFICATION 
The subject of procurement is not divided into groups. The tenderer is obliged to submit a tender that includes the total subject of procurement as defined in the technical specifications.
Table 3_Techincal specification and quantities

	Mobile plant for the production of ready-mixed concrete, 1 set

	Name of the machine (model, type)
	

	No.
	Required specification
	Required value
	Offered value

	0.
	Mobile plant capacity for the delivery of fresh concrete
	Min. 90 m³/h
	

	1. Mixer

	1.1.
	Mixer volume
	Min. 2,0 m³
	

	1.2.
	Engine power
	Min. 37 kW
	

	2. Cement weightbridge

	2.1.
	Allowed load
	Min. 1000 kg
	

	2.2.
	Calibration and certification
	YES
	

	3. Complete control and management system

	3.1.
	OPERATOR CABIN with all ICT equipment for control, management and printing of the documents (computer, printer, etc.)
	YES
	

	3.2.
	Cabin dimensions
	Min. 1,8 x 2 m
	

	3.3.
	Control software
	YES
	

	3.4.
	Operating regime
	automatic, manual, combined
	

	3.5.
	PLC
	YES
	

	4. Electroinstallation

	4.1.
	Complete cabling for all drive DEVICES, LIMIT SWITCHES AND DISTRIBUTORS
	YES
	

	5.  Aggregate bunkers

	5.1.
	Number of bunkers
	5 pieces
	

	5.2.
	Single bunker volume capacity
	min. 6 m³, max. 25 m³
	

	5.3.
	Fine dosage option
	YES
	

	5.4.
	Aggregate transfer belt
	Width of belt
Min. 800 mm

Allowed load
Min.  2.500 kg

Calibration and certification

YES


	Width of belt

Allowed load

Calibration and certification



	5.5.
	Pneumatics
	YES
	

	5.6.
	Compressor for pneumatics installation
	YES
	

	6. Cement silo to cement weighbridge transporter (screw conveyor)

	6.1.
	CAPACITY
	Min. 32 m3/h
	

	7. Cement silo

	7.1.
	Capacity
	Min. 100 t
	

	7.2.
	Filter
	YES
	

	8. Other parts

	8.1.
	WATER WEIGHBRIDGE with calibration and certification
	YES
	

	8.2.
	ADDITIVE WEIGHBRIDGE with calibration and certification
	YES
	

	8.3.
	INDEPENDENT POWER SOURCE – power generator
	Output power

Must be enough to run the overall offered plant, but min. 250 kVa
Is mobile 

YES

Sound insulation

YES

Own fuel tank

YES


	Output power

Is mobile 

Sound insulation

Own fuel tank



	9. Other conditions

	9.1.
	Guarantee for repair of defects in the guarantee period
	YES, Min. 12 months after the installation
	

	9.2.
	Training for the 3 workers
	YES
	

	9.3.
	First montage and testing the production
	YES
	

	9.4.
	Facility colour
	RAL 2011
	

	9.5.
	Conformity with DIRECTIVE 2006/42/EC OF THE EUROPEAN PARLIAMENT AND OF THE COUNCIL
	YES
	


	Total value, excluding VAT:
	

	VAT:
	

	Total value, with VAT:
	


Table 4_List of main deliveries

	LIST OF MAIN DELIVERIES

	No.
	Name and/or description of delivery
	Date of delivery
	Name of the other contracting party

	Amount of delivery without VAT in 

HRK / EUR (circle the currency)

	1.
	
	
	
	

	2.
	
	
	
	

	3.
	
	
	
	

	4.
	
	
	
	

	5.
	
	
	
	

	TOTAL:
	


                                                                TENDERER:
Date:  ________________                               (Stamp)                                                        _____________________________________________

                                                                                                    (Signature of the authorised person of the tenderer)
7
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