PRILOG IV. / ANNEX IV.
TEHNIČKE SPECIFIKACIJE / TEHNICAL SPECIFICATIONS
Ev. broj nabave / Procurement number: 01/2022

NAZIV NABAVE / Name of procurement: Nabava automatske punilice za limenke / Procurement of automatic can filler

NAPOMENA: Ponuditelj nudi predmet nabave putem ove tablice Tehničkih specifikacija koja će činiti dio ponude.
Ponuditelj je dužan ponuditi svaku stavku kako je tražena u stupcu 2. Tražene karakteristike.
Ponuđeni predmet nabave je pravilan i prihvatljiv samo ako ispunjava sve zahtijevane uvjete i svojstva. Nije prihvatljivo precrtavanje ili korigiranje stavke navedene u stupcu 2. Tražene karakteristike. Ponuditelj obavezno popunjava stupac 3. «Ponuđene karakteristike» definirajući detaljno tehničke specifikacije ponuđene robe.
NOTE: These Technical specifications must be filled in by the tenderer and will be submitted as a part of the tender.
The tenderer is obliged to offer each item as required in column 2. Required technical specification.
Offered item is acceptable only if it meets all the required conditions and properties. No amendments or corrections to the items listed in column 2. Required technical specification are allowed. Tenderer is required to fill column 3 " Offered technical specification " defining in detail the technical specifications of the goods offered.

	1. Red. br. / No.
	2. Tražene karakteristike / Required technical specifications
	3. Ponuđene karakteristike / Offered technical specifications

	1.
	AUTOMATSKA PUNILICA ZA LIMENKE / AUTOMATIC CAN FILLER

	1.1
	Kapacitet: minimalno 2.000 limenki na sat /
Capacity: minimum 2,000 cans per hour
	

	1.2
	Dodatni prilagodni set za 3 veličine limenki (250ml, 330ml i 500ml) /
Additional adjustment set for 3 sizes of cans (250ml, 330ml and 500ml)
	

	1.3
	Automatski depaletizer /
Automatic depalletizer
	

	1.4
	Nitro dozer / 
Nitro dozer
	

	1.5
	Stol za skupljanje napunjenih limenki /
Table for collecting filled cans
	

	1.6
	Instalacija i puštanje u pogon /
Installation and commissioning
	

	1.7
	Trajanje jamstvenog roka (minimalno 12 mjeseci) /
Warranty period (minimum 12 months)
	

	
	PROIZVOĐAČ I MODEL /
MANUFACTURER AND MODEL:
	




U / In _______________________________, ___________2022.

____________________________________________
(ime, prezime i potpis osobe ovlaštene za zastupanje gospodarskog subjekta / name, surname and signature of the person authorized to represent the economic operator)
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